auto lo
iface lo inet loopback

# TODO: only configure eth0 interfaz
auto eth0
iface eth0 inet dhcp
	hwaddress ether 00:00:00:00:00:01

##
## Don't edit the text below.

auto eth1
iface eth1 inet static
	address 121.13.8.1
	netmask 255.255.252.0

up route add default gw 121.13.8.2