auto lo
iface lo inet loopback

# TODO: only configure eth0 interfaz
auto eth0
iface eth0 inet dhcp
	hwaddress ether 00:00:00:00:00:01

##
## Don't edit the text below.

auto eth1
iface eth1 inet static
	address 17.21.100.1
	netmask 255.255.255.0

auto eth2
iface eth2 inet static
	address 32.8.10.1
	netmask 255.255.255.0

